**VEHICLE SPECIFICATIONS ALL CLASSES 2020**

* 4 wheel steering is not permitted
* Soft top or open top vehicles must have rollover protection – factory or after market.
* The decision to start, continue or finish a track resides with the driver of the competing vehicle.
* Current Third Party Extension must be presented at scrutineering, unless vehicle is unregistered.
* Fully operational restraint systems must be in place. – (seat belts)
* Vehicles must have a fire extinguisher in working order and easily accessible.
* Visible and working reversing lights.
* Must have snatch strap and two rated shackles.
* Front and rear recovery points.
* No agricultural type tyres or tyre chains are allowed.
* Body lift permitted.
* Spring lift permitted, but classified by size in each of the classes.
* Driver and Navi to wear helmets, Gloves to be worn when outside the vehicle.
* 10 minute time limit per track. .ie you have 10 minutes to complete the track.

**STANDARD CLASS**

* No reduction gears. **Vehicles must be registered and obtain**
* Maximum tyre size up to and including 33 inch. **3rd Party extension Insurance for the comp.**
* No diff locks allowed.
* Vehicles fitted with lockers must have them disconnected.
* No tyre bead locking devises allowed.
* No wheel spacers.
* No drop shackles allowed.
* Standard spring and diff mounting points only.
* Window nets to be fitted to both Driver’s and Navi’s doors, or window to remain closed at least 50% or greater than the window opening.
* Maximum lift is to be 4 inches.

**LOCKED CLASS**

* Maximum tyre size up to and including 35 inch. **Vehicles must be registered and obtain**
* Diff locks permitted. **3rd** **Party extension** **Insurance for the comp.**
* Single transfer case only.
* Reduction gears not allowed – or 100 point penalty.
* No tyre bead locking device allowed – or 100 point penalty.
* No wheel spacers allowed.
* No Exo cages allowed.
* Standard factory spring and diff mounts points only.
* No drop shackles allowed.
* Window net fitted to both Driver’s and Navi’s doors.
* Maximum lift is to be 4 inches.

**MODIFIED CLASS**

* Maximum tyre size up to and including 37 inch**. Must carry first aid kit in vehicle at all times**.
* Diff lock permitted. **Must have a fire extinguisher.**
* Dual transfer cases allowed**. Internal kill switch required.**
* Reduction gears allowed. **Vehicle registration not required**
* Bead locking devices allowed.
* Wheel spacers allowed.
* Drop shackles allowed.
* Window net fitted to both Driver’s and Navi’s doors.
* Hydro steering NOT allowed.
* Maximum lift is to be 6 inches.
* Must have 80% or more original chassis, panels can be modified.
* Suspension - no limit.

**VEHICLE SPECIFICATIONS ALL CLASSES 2020**

**BUGGY CLASS**

* Maximum tyre size up to and including 40 inch**. Must carry first aid kit in vehicle at all times**.
* Diff lock permitted. **Must have a fire extinguisher.**
* Dual transfer cases allowed. **Internal kill switch required.**
* Reduction gears allowed. **Vehicle registration not required**
* Bead locking devices allowed.
* Wheel spacers allowed.
* Diff and spring - no limit
* Drop shackles allowed.
* Window net fitted to both Driver’s and Navi’s doors.
* Hydro steering allowed.
* Must have internal or external roll cage.
* Front Digs allowed.
* No Rear steer – If used penalty per track 50 points.
* Tube frame allowed.